D_80AEF800 {
    //! Uses long command, even when it isn't required
    if_time_range_l (6, 0, 18, 0) {
        return_time (6, 0, 18, 0, 1)
        //! trailing return
        return_none
    } else {
        return_none
    }
}
