/*
 * MPC8544 DS Device Tree Source
 *
 * Copyright 2007, 2008 Freescale Semiconductor Inc.
 *
 * This program is free software; you can redistribute  it and/or modify it
 * under  the terms of  the GNU General  Public License as published by the
 * Free Software Foundation;  either version 2 of the  License, or (at your
 * option) any later version.
 */

/dts-v1/;
/ {
	model = "MPC8544DS";
	compatible = "MPC8544DS", "MPC85xxDS";
	#address-cells = <1>;
	#size-cells = <1>;

	aliases {
		serial0 = &serial0;
		serial1 = &serial1;
		pci0 = &pci0;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		PowerPC,8544@0 {
			device_type = "cpu";
			reg = <0x0>;
			d-cache-line-size = <32>;	// 32 bytes
			i-cache-line-size = <32>;	// 32 bytes
			d-cache-size = <0x8000>;		// L1, 32K
			i-cache-size = <0x8000>;		// L1, 32K
			timebase-frequency = <0>;
			bus-frequency = <0>;
			clock-frequency = <0>;
		};
	};

	memory {
		device_type = "memory";
		reg = <0x0 0x0>;	// Filled by U-Boot
	};

	soc8544@e0000000 {
		#address-cells = <1>;
		#size-cells = <1>;
		device_type = "soc";
		compatible = "simple-bus";

		ranges = <0x0 0xe0000000 0x100000>;
		reg = <0xe0000000 0x1000>;	// CCSRBAR 1M
		bus-frequency = <0>;		// Filled out by uboot.

		serial0: serial@4500 {
			cell-index = <0>;
			device_type = "serial";
			compatible = "ns16550";
			reg = <0x4500 0x100>;
			clock-frequency = <0>;
			interrupts = <42 2>;
			interrupt-parent = <&mpic>;
		};

		serial1: serial@4600 {
			cell-index = <1>;
			device_type = "serial";
			compatible = "ns16550";
			reg = <0x4600 0x100>;
			clock-frequency = <0>;
			interrupts = <42 2>;
			interrupt-parent = <&mpic>;
		};

		mpic: pic@40000 {
			interrupt-controller;
			#address-cells = <0>;
			#interrupt-cells = <2>;
			reg = <0x40000 0x40000>;
			compatible = "chrp,open-pic";
			device_type = "open-pic";
		};

                global-utilities@e0000 {        //global utilities block
                        compatible = "fsl,mpc8544-guts";
                        reg = <0xe0000 0x1000>;
                        fsl,has-rstcr;
                };
	};

	pci0: pci@e0008000 {
		cell-index = <0>;
		compatible = "fsl,mpc8540-pci";
		device_type = "pci";
		interrupt-map-mask = <0xf800 0x0 0x0 0x7>;
		interrupt-map = <

			/* IDSEL 0x11 J17 Slot 1 */
			0x8800 0x0 0x0 0x1 &mpic 0x2 0x1
			0x8800 0x0 0x0 0x2 &mpic 0x3 0x1
			0x8800 0x0 0x0 0x3 &mpic 0x4 0x1
			0x8800 0x0 0x0 0x4 &mpic 0x1 0x1

			/* IDSEL 0x12 J16 Slot 2 */

			0x9000 0x0 0x0 0x1 &mpic 0x3 0x1
			0x9000 0x0 0x0 0x2 &mpic 0x4 0x1
			0x9000 0x0 0x0 0x3 &mpic 0x2 0x1
			0x9000 0x0 0x0 0x4 &mpic 0x1 0x1>;

		interrupt-parent = <&mpic>;
		interrupts = <24 2>;
		bus-range = <0 255>;
		ranges = <0x2000000 0x0 0xc0000000 0xc0000000 0x0 0x20000000
			  0x1000000 0x0 0x0 0xe1000000 0x0 0x10000>;
		clock-frequency = <66666666>;
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		reg = <0xe0008000 0x1000>;
	};

	chosen {
		linux,stdout-path = "/soc8544@e0000000/serial@4500";
	};

	hypervisor {
	};
};
